Video playback applications in Dual Head mode produce an error message or fail to start This information applies to the following system configurations: AMD Proprietary Linux Driver version 3.14.6 and earlier AMD display adapter with Dual Head capability X Server Dual Head configuration The following may occur during the execution of a video playback application: fails to start video playback error This does not apply to Single Head X Server configurations. This issue has been resolved in the 8.8.25 driver.